For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement.

1 | Digital Radio Receiver Assembly Tip

• | Disconnect the electrical connectors.

• | Perform the digital radio receiver set up procedure. Refer to Control Module References for programming and setup information.

2 | Digital Radio Receiver Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)