For 1990-2009 cars

## Body Side Molding Replacement Sedan

Callout | Component Name
--- | ---

#### Special Tools

J 25070 Heat Gun 500-750°F

1 | Body Side Molding - Front Door Tip

• | The body side front door molding is attached using double sided tape. Use J 25070 or equivalent to aid in removal.

• | If the molding is missing, take dimensions from the other side of the vehicle for proper location.

2 | Body Side Molding - Rear Door Tip

• | The body side rear door molding is attached using double sided tape. Use J 25070 or equivalent to aid in removal.

• | If the molding is missing, take dimensions from the other side of the vehicle for proper location.

## Body Side Molding Replacement Coupe

Callout | Component Name
--- | ---

#### Special Tools

J 25070 Heat Gun 500-750°F

1 | Body Side Molding (Door) Tip

• | The body side door molding is attached using double sided tape. Use J 25070 or equivalent to aid in removal.

• | If the molding is missing, take dimensions from the other side of the vehicle for proper location.

2 | Body Side Molding - Quarter Panel Tip

• | The body side quarter panel molding is attached using double sided tape. Use J 25070 or equivalent to aid in removal.

• | If the molding is missing, take dimensions from the other side of the vehicle for proper location.