For 1990-2009 cars

#### Special Tools

J 36850 Assembly Lubricant

For equivalent regional tools, refer to Special Tools.

1. Assemble the forward clutch hub (577) onto the input internal gear (560) and retain it with the snap ring (578).
2. Assemble the thrust washer (109) onto the forward clutch hub (577) with the thrust washer tabs toward the forward clutch hub (577). Retain the thrust washer with J 36850 lubricant or equivalent.