For 1990-2009 cars

Table 1: | Gear Teeth Counts and Ratios
Table 2: | Blocking Ring Clearances
Table 3: | Axial Play Specifications

#### Gear Teeth Counts and Ratios

Gear | Gear Teeth Count
--- | ---
1st Drive | 13
1st Driven | 44
2nd Drive | 25
2nd Driven | 44
3rd Drive | 39
3rd Driven | 46
4th Drive | 47
4th Driven | 42
5th Drive | 54
5th Driven | 38
Reverse Drive | 25
Reverse Idler | 21
1st & 2nd Gear Synchronizer Sleeve | 49
Output Shaft | 20
Ring Gear | 89

#### Blocking Ring Clearances

Measure | Standard | Service Limit
--- | --- | ---
Metric | English | Metric | English
1st and 2nd Gears | 1.2-1.4 mm (min.) | 0.047-0.055 in (min.) | 0.8 mm (min.) | 0.032 in (min.)
3rd, 4th, and Reverse Gears | 0.9-1.2 mm (min.) | 0.035-0.047 in (min.) | 0.5 mm (min.) | 0.020 in (min.)
5th Gear | 0.7-1.1 mm (min.) | 0.028-0.043 in (min.) | 0.5 mm (min.) | 0.020 in (min.)

#### Axial Play Specifications

Measurement | Specification
--- | ---
Metric | English
Between 2nd and 3rd Drive Gears | 0.05-0.40 mm | 0.002-0.016 in
Between 4th Drive Gear and Input Shaft Bearing | 0.05-0.40 mm | 0.002-0.016 in
Between Reverse Gear and Reverse Gear Washer | 0.10-0.20 mm | 0.004-0.008 in
Input Shaft Axial Play | 0.09-0.15 mm | 0.004-0.006 in
Output Shaft Axial Play | This is a calculated value. It can change based upon age of case and output shaft bearing. Refer to Transmission Assemble .