For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
2. Disconnect the inlet and outlet pipes to the charge air cooler. Refer to Charge Air Cooler Inlet Pipe Replacement and Charge Air Cooler Outlet Pipe Replacement.

1 | Charge Air Cooler Bolt (Qty:4) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Charge Air Cooler