For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the headlamp assembly. Refer to Headlamp Replacement.

1 | Headlamp Bracket Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 9 N·m (80 lb in)
2 | Headlamp Bracket

#### Procedure

1. Pull the bracket from the backside of the headlamp assembly.
2. Inspect the two J-clips, replace if damaged.
3. Upon installation of the bracket to the headlamp, the lower edge of the bracket must engage to the two clips on the bottom side of the headlamp prior to bolt installation.