For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner outlet duct .
2. Remove the air cleaner assembly attachment fasteners.
3. Remove the air cleaner.

### Installation Procedure

Important: Verify full engagement of the inlet onto the resonator neck.

1. Position the air cleaner assembly.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the air cleaner assembly attachment bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

3. Connect the air cleaner resonator to the air cleaner assembly.

Tighten
Tighten the air cleaner outlet duct clamps to 5 N·m (44 lb in).