For 1990-2009 cars

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. When testing the circuit for a high resistance, ensure to use the voltage drop test in the Circuit Testing procedure. If the circuit has more than more than a 0.5-volt drop when the starter is engaged then there is a high resistance.

2. When testing the circuit for a high resistance, ensure to use the voltage drop test in the Circuit Testing procedure. If the circuit has more than a 0.5-volt drop when the starter is engaged, then there is a high resistance. Ensure when testing the engine ground to battery to connect the engine ground lead to the base of the starter.

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Starting and Charging Schematics
1 | Did you perform the Diagnostic System Check - Vehicle? | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 | Turn the ignition to the START position. Did the starter solenoid click? | Go to Step 3 | Go to Starter Solenoid Does Not Click
3 | Inspect the engine and belt drive system for mechanical binding, e.g. seized engine, seized generator. Does the engine move freely? | Go to Step 4 |

• | Go to Engine Will Not Crank - Crankshaft Will Not Rotate for the 2.0L engine

• | Go to Engine Will Not Crank - Crankshaft Will Not Rotate for the 2.2L (L61) engine

• | Go to Engine Cranks But Does Not Run for the 2.4L engine

4 | Test the battery positive cable between the battery and the starter solenoid for high resistance. Refer to Circuit Testing and Wiring Repairs . Did you find and correct the condition? | Go to Step 8 | Go to Step 5
5 | Test the ground circuit between the battery and the engine for a high resistance. Refer to Circuit Testing and Wiring Repairs . Did you find and correct the condition? | Go to Step 8 | Go to Step 6
6 | Inspect for poor connections at the starter. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs . Did you find and correct the condition? | Go to Step 8 | Go to Step 7
7 | Replace the starter. Refer to Starter Motor Replacement . Did you complete the replacement? | Go to Step 8 | --
8 | Operate the system for which the symptom occurred. Did you correct the condition? | System OK | Go to Step 2