For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Catalytic Converter-to-Exhaust Manifold Nuts | 50 N·m | 37 lb ft
Catalytic Converter-to-Muffler Pipe Nut | 30 N·m | 22 lb ft
Exhaust Clamp Nut | 45 N·m | 33 lb ft
Exhaust Manifold Heat Shield Stud | 22 N·m | 16 lb ft
Exhaust Manifold Nut | 14 N·m | 10 lb ft
Heater Oxygen Sensor (HO2S) | 42 N·m | 31 lb ft
Heat Shield Nut | 10 N·m | 89 lb in
Positive Crankcase Ventilation (PCV) Vent Tube Bolt/Nut (RPO LSJ) | 10 N·m | 89 lb in
Secondary Air Injection (AIR) Outlet Hose/Pipe Bracket Bolt (RPO L61) | 20 N·m | 15 lb ft
Secondary Air Injection (AIR) Outlet Hose/Pipe Bracket Nut (RPO L61) | 10 N·m | 89 lb in
Wheel Drive Shaft Heat Shield Bolt (to Engine Block) | 30 N·m | 22 lb ft
Wheel Drive Shaft Heat Shield Bolt (to Transaxle Mount Bracket) | 10 N·m | 89 lb in