For 1990-2009 cars

### Removal Procedure

1. With a flat-bladed tool, separate the outer trim cover from the instrument panel (I/P).
2. Pull the outer trim cover rearward from the I/P to disengage the locating tabs.
3. Remove the outer trim cover from the I/P.

### Installation Procedure

1. Align the outer trim cover locating tabs to the opening in the I/P.
2. Push the outer trim cover locating tabs into the I/P until fully engaged.
3. Press the outer trim cover into the I/P until fully secured.