For 1990-2009 cars

## Radiator Upper Grille Replacement Cobalt SS Turbo

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.

1 | Energy Absorber Retainer (Qty: 2)
2 | Radiator Grille Emblem Nut (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 1.5 N·m (13 lb in)
3 | Radiator Upper Grille Tip Release the front bumper fascia tabs from the upper grille assembly in order to remove.