For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement.

1 | Steering Wheel Horn Contact Bolt (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 8 N·m (71 lb in)
2 | Steering Wheel Horn Contact

#### Procedure

Disconnect any electrical connectors as needed.

3 | Steering Wheel Nut Tighten 40 N·m (30 lb ft)
4 | Steering Wheel

#### Procedure

1. Use puller J 1859-A and puller legs J 42578 to remove the steering wheel.
2. Disconnect any electrical connectors as needed.

#### Special Tools

• | J 1859-A Steering Wheel Puller

• | J 42578 Steering Wheel Puller Legs