For 1990-2009 cars

### Removal Procedure

Warning: Refer to Brake Dust Warning in the Preface section.

1. Remove the brake drum. Refer to Brake Drum Replacement.
2. Remove the brake adjuster actuator lever spring (1).
3. Remove the brake adjuster actuator lever (1).
4. Remove the brake shoe hold down spring and cup (1) assemblies by compressing the spring and rotating the assembly ¼ turn.
5. Remove the 2 hold down spring and cup assembly pins.
6. Spread the top of the brake shoes apart slightly and remove the brake shoe adjuster (1).
7. Inspect the drum brake adjusting hardware and replace any components, as necessary. Refer to Drum Brake Adjusting Hardware Inspection.
8. Remove the upper brake shoe return spring (1).
9. Rotate the primary brake shoe (1) toward the wheel hub assembly and release the brake shoe from the lower brake shoe return spring.
10. Remove the lower brake shoe return spring (1).
11. Inspect the drum brake hardware and replace any components, as necessary. Refer to Drum Brake Hardware Inspection.
12. Compress the park brake cable return spring and release the park brake cable fitting (1) from the park brake apply lever and remove the brake shoe (2).

### Installation Procedure

1. Clean the drum brake backing plate of any dirt and debris.
2. Apply a light coat of high temperature brake lubricant to the drum brake backing plate brake shoe contact surfaces.
3. Compress the park brake cable return spring and install the park brake cable fitting (1) to the park brake apply lever and position the brake shoe (2) to the drum brake backing plate.
4. Install the lower brake shoe return spring (1).
5. Position the primary brake shoe (1) to the drum brake backing plate and connect the brake shoe to the lower brake shoe return spring.
6. Install the upper brake shoe return spring (1).
7. Spread the top of the brake shoes apart slightly and install the brake shoe adjuster (1).
8. Install the 2 hold down spring and cup assembly pins.
9. Install the brake shoe hold down spring and cup (1) assemblies by compressing the spring and rotating the assembly ¼ turn.
10. Install the brake adjuster actuator lever (1).
11. Install the brake adjuster actuator lever spring (1).
12. Adjust the drum brakes. Refer to Drum Brake Adjustment.
13. Install the brake drum. Refer to Brake Drum Replacement.