For 1990-2009 cars

#### Tools Required

J 22610 Keystone Clamp Pliers

### Removal Procedure

1. Remove the rack and pinion outer tie rod end. Refer to Rack and Pinion Outer Tie Rod End Replacement .
2. Remove the rack and pinion inner tie rod nut and discard it.
3. Remove the outer steering gear boot clamp.
4. Cut the inner steering gear boot clamp and discard it.

Important: After removing the boot, inspect the inner tie rod for evidence of corrosion or contamination. If none is evident, continue with the repair. If corrosion or contamination is evident, replace the steering gear.

5. Remove the steering gear boot from the steering gear.

### Installation Procedure

1. Install a new inner steering gear boot clamp on the steering gear boot.

Important: Inspect the steering gear and the rack and pinion inner tie rod for any debris. The parts must be clean and free of debris before installing the steering gear boot.

2. Apply grease from the steering gear boot service kit to the indicated locations.

Important: The steering gear boot must seat in the groove on the steering gear.

3. Install the steering gear boot to the steering gear.
4. Use pliers J 22610 to crimp the inner steering gear boot clamp.
5. Install the outer steering gear boot clamp.
6. Install a new rack and pinion inner tie rod nut.
7. Install the rack and pinion outer tie rod end. Refer to Rack and Pinion Outer Tie Rod End Replacement .
8. Adjust the front toe. Refer to Front Toe Adjustment .