For 1990-2009 cars

### Removal Procedure

1. Remove the right front tire and wheel. Refer to Tire and Wheel Removal and Installation .
2. Remove the right front fender liner. Refer to Front Fender Liner Replacement .
3. Remove the air cleaner intake duct retainer.
4. Remove the air cleaner intake duct bolt.
5. Remove the air cleaner intake duct.

### Installation Procedure

1. Position the air cleaner intake duct.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the air cleaner intake duct bolt.

Tighten
Tighten the bolt to 10 N·m (89 lb ft).

3. Install the air cleaner intake duct retainer.
4. Install the right front fender liner. Refer to Front Fender Liner Replacement .
5. Install the right front tire and wheel. Refer to Tire and Wheel Removal and Installation .