For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Charge Air Bypass Valve Solenoid Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Charge Air Bypass Solenoid Vacuum Hose Clamp (Qty: 3)

#### Procedure

Reposition the clamps in order to remove the hoses.

Tip
Note the hose locations for proper reinstallation.

3 | Charge Air Bypass Valve Solenoid

#### Procedure

Disconnect the electrical connector.