For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the wheel drive shaft heat shield bolt at the transaxle mount bracket.
3. Remove the drive shaft heat shield bolt at the engine block.
4. Remove the wheel drive shaft heat shield.

### Installation Procedure

1. Install the wheel drive shaft heat shield into position on the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the wheel drive shaft heat shield bolt to the engine block and tighten the bolt to 30 N·m (22 lb ft).
3. Install the wheel drive shaft heat shield bolt to the transaxle mount bracket and tighten the bolt to 10 N·m (89 lb in).
4. Lower the vehicle.