For 1990-2009 cars

### Removal Procedure

1. Pull the hood rear seal from the air inlet grille panel to remove it.
2. Remove the wiper arms. Refer to Windshield Wiper Arm Replacement .
3. Remove the push pin fasteners in the air inlet grille panel.
4. Disconnect the washer fluid hose.
5. Remove the air inlet grille panel from the vehicle.
6. Remove the washer nozzles from the air inlet grille panel.

### Installation Procedure

1. Install the washer nozzles to the air inlet grille panel.
2. Position the air inlet grille panel to the vehicle.
3. Connect the washer fluid hose.
4. Install the push pin fasteners to the air inlet grille panel.
5. Install the wiper arms. Refer to Windshield Wiper Arm Replacement .
6. Install the hood rear seal to the air inlet grille panel and press it into position.