For 1990-2009 cars

### Removal Procedure

1. Disconnect the evaporative emission (EVAP) canister purge valve harness connector.
2. Disconnect the vacuum pipe from the EVAP canister purge valve.
3. Disconnect the purge pipe from the EVAP canister purge valve.
4. Remove the EVAP canister purge valve and bracket.
5. Remove the EVAP canister purge valve from the purge bracket.
6. Inspect for carbon release in the EVAP canister purge valve ports. Refer to Evaporative Emission System Cleaning .

### Installation Procedure

1. Install the EVAP canister purge valve on to the purge bracket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the EVAP canister purge valve and bracket.

Tighten
Tighten the purge bracket nut to 8 N·m (71 lb in).

3. Connect the purge pipe to the EVAP canister purge valve.
4. Connect the vacuum pipe to the EVAP canister purge valve.
5. Connect the EVAP canister purge valve harness connector.