For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the steering column opening filler assembly. Refer to Steering Column Opening Filler Replacement.
2. Tilt the steering wheel up.

1 | Instrument Panel Trim Tip

• | Release the left-hand instrument panel (I/P) trim plate assembly by pulling away from the I/P retainer.

• | Disconnect the I/P dimmer switch and, if equipped, the fog lamp switch.

2 | I/P Trim Panel Clip