For 1990-2009 cars

## Windshield Wiper Blade Replacement Pontiac Coupe

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Lift the wiper arm from the windshield to the service up position.
2. Release the wiper blade finish cover and rotate the cover rearward towards the wiper arm.
3. Release the lock securing the wiper arm sheep hook to the blade assembly.
4. Pull the blade assembly rearward in order to release the sheep hook from the blade.
5. Push the blade assembly away from the arm, through the finish cover.

1 | Wiper Blade Finish Cover Tip Lift and rotate the forward edge of the cover and leave the cover attached to the wiper blade assembly.
2 | Wiper Blade Assembly

## Windshield Wiper Blade Replacement Chevrolet Coupe, Sedan

### Removal Procedure

1. Move the wiper arm to the service up position
2. Press the wiper blade clip button in to release the wiper blade from the inside radius of the wiper arm.
3. Remove the wiper blade out through the opening in the wiper arm.

### Installation Procedure

1. Install the hook of the wiper arm through the opening in the wiper blade.
2. Press the wiper blade pivot into the wiper arm hook until the pivot locks into the hook.
3. Position the wiper blade pivot in the inside radius of the wiper arm hook.
4. Move the wiper arm back to the parked position.
5. Operate the windshield wipers and inspect for proper operation.