For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Rear Side Door Trim Panel Replacement.
2. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement.
3. Move the window to the full up position and secure in place with tape.

1 | Side Door Window Regulator Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tip Loosen the bolts enough so that the regulator assembly will lift out of the t-slots in the door inner panel. Tighten
10 N·m (89 lb in)

2 | Rear Side Door Window Regulator Assembly
3 | Rear Side Door Window Regulator Motor Tip Disconnect the electrical connector.