For 1990-2009 cars

#### Tools Required

• | J 38122-A Harmonic Balancer Holder

• | J 45059 Angle Meter

### Removal Procedure

1. Remove the drive belt. Refer to Drive Belt Replacement .
2. Use J 38122-A to prevent the crankshaft from rotating while loosening the crankshaft balancer bolt.
3. Remove and discard the crankshaft balancer bolt.
4. Remove the crankshaft balancer.

### Installation Procedure

1. Position the crankshaft balancer.
2. Install a NEW crankshaft balancer bolt.
3. Use the J 38122-A to hold the crankshaft balancer in order to prevent the balancer from rotating while tightening the bolt.

Notice: Refer to Fastener Notice in the Preface section.

4. Tighten the crankshaft balancer bolt.

Tighten
Tighten the bolt to 100 N·m (74 lb ft) plus an additional 125 degrees using the J 45059 .

5. Install the drive belt. Refer to Drive Belt Replacement .