For 1990-2009 cars

### Removal Procedure

1. Remove the left front wheel. Refer to Tire and Wheel Removal and Installation.
2. Disconnect the vehicle speed sensor (VSS) electrical connector (2).
3. Remove the retainer bolt.
4. Remove the retainer.
5. Remove the VSS.
6. Remove and discard the O-ring.

### Installation Procedure

1. Lubricate a new O-ring with transmission fluid. Refer to Lubrication Specifications.
2. Install the new O-ring.
3. Install the VSS retainer.

Install the VSS assembly.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the VSS retainer bolt and tighten to 9 N·m (80 lb in).
5. Connect the VSS connector to the VSS (2).
6. Install the left front wheel. Refer to Tire and Wheel Removal and Installation.