For 1990-2009 cars

## Clutch Pedal Position Switch Adjustment Old Pedal

### Removal Procedure

1. Remove the steering column. Refer to Steering Column Replacement .
2. Disconnect the electrical connector (2) from the clutch pedal position (CPP) switch (1).
3. Remove the CPP switch (1) from the clutch pedal by twisting the CPP switch (1) counterclockwise.

### Installation Procedure

1. A 3/32 inch or 2 mm drill bit can be used as a gage tool for the proper adjustment of the CPP switch. Insert and seat the 3/32 inch or 2 mm drill bit through the slot in the top of the clutch pedal assembly.
2. Install the CPP switch (1) to the clutch pedal assembly.
3. While holding the pedal in the fully released position, press the switch (1) toward the pedal until the barrel of the switch touches the drill bit on the pedal assembly.
4. Rotate the switch (1) clockwise to secure.
5. Remove the drill bit.
6. Connect the electrical connector (2) to the CPP switch (1).
7. Install the steering column. Refer to Steering Column Replacement .

## Clutch Pedal Position Switch Adjustment New Pedal

### Installation Procedure

1. Remove the steering column. Refer to Steering Column Replacement .
2. While holding the pedal in the fully released position, press the switch (2) toward the pedal until the barrel of the switch (2) touches the shipping clip (1).
3. Rotate the switch (1) clockwise to secure.
4. Remove the shipping clip (1).
5. Connect the electrical connector (3).
6. Install the steering column. Refer to Steering Column Replacement .