For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the front transaxle mount thru bolt.
3. Remove the front transaxle mount to transaxle bolts.
4. Remove the front transaxle mount from the vehicle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Important: The transaxle bolts must be torqued in a mandatory sequence as shown.

1. Install the front transaxle mount and transaxle bolts.

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

2. Hand start the front transaxle mount through bolt.

Important: The front and rear transaxle mounts must be allowed to settle with the through bolts loosened.

3. Loosen the rear transaxle mount through bolt.
4. Tighten the transaxle mount through bolts in the following order:

Tighten

1. Tighten the rear bolt to 100 N·m (74 lb ft).
2. Tighten the front bolt to 100 N·m (74 lb ft).

5. Lower the vehicle.