For 1990-2009 cars

### Removal Procedure

1. Remove the drive belt. Refer to Drive Belt Replacement .
2. Remove the drive belt tensioner bolt.
3. Remove the drive belt tensioner.

### Installation Procedure

1. Position the drive belt tensioner.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the drive belt tensioner bolt.

Tighten
Tighten the bolt to 45 N·m (33 lb ft).

3. Install the drive belt. Refer to Drive Belt Replacement .