TPS ADJUSTMENT CORRECTION PROCEDURE ERROR (MANUAL). Pontiac J2000 1983

For 1990-2009 cars

# TPS ADJUSTMENT CORRECTION PROCEDURE ERROR (MANUAL)

#### VEHICLES AFFECTED: 1983 & 1984 'J' Models Equippeci With 2.0L LQ5 Engine (VIN Code 'P')

Step 4 of the Throttle Position Sensor Adjustment Procedure shown on Page 6C15-5 of the 1983 Divisional Shop Manuals and on Page 6C15-4 of the 1984 Divisional Shop Manuals is in error. The voltage should be measured between terminals A and B, not B and C as presently shown.

Please make a note of this in your copies of the shop manuals.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.