LABOR OPERATIONS FOR SUNBIRD CONVERTIBLE TOP. Pontiac J2000 1983

For 1990-2009 cars

# LABOR OPERATIONS FOR SUNBIRD CONVERTIBLE TOP

LABOR OPERATIONS FOR 1983 2000 SUNBIRD CONVERTIBLE TOP

Listed below are labor operations to be used when performing warranty work on 1983 2000 Sunbird convertible tops.

LABOR OPERATION TIME LABOR OPERATION DESCRIPTION NUMBER ALLOWANCE

Applique, Front Header (Exterior) - R&R Or Replace ..... B3000 1.4

Molding, Front Header Lock Replace Right .......................................... B3020 .2 Left .......................................... B3021 .2

Molding, Front Header - Replace ........................ B3040 .5

Applique, Windshield Header (Interior Trim - Replace) .. B3060 .4

Seal Assembly, Front (Header Weatherstrip) - Replace ... B3070 .4

Seal, Front To Center Rail - Replace Right ........................................... B3090 .2 Left ........................................... B3091 .2

Seal, Center To Rear Rail - Replace Right............................................ B3110 .2 Left............................................. B3111 .2

Seal, Center Rail (Center Roof Rail Weatherstrip) - Replace Right............................................ B3130 .2 Left............................................. B3131 .2

Seal, Rear Rail (Reat Roof Rail Weatherstrip) - Replace Right............................................ B3150 .2 Left............................................. B3151 .2

Pin, Dowel - Replace Right............................................ B3220 .2 Left............................................. B3221 .2 Latch, Replace Right............................................ B3240 .2 Left............................................. B3241 .2 Clamp Assembly (Lock Handle) - Replace Right............................................ B3260 .3 Left............................................. B3261 .3 Cable Side Retention - Replace Right............................................ B3360 .2 Left............................................. B3361 .2 Cvlinder, Folding Top Lift - Replace (Inc: Bleed And Refill System) Right............................................ B3420 .8 Left............................................. B3421 .8 Motor And Pump Assembly Replace......................... B3460 .9 (Inc: Bleed And Refill System) Welt Assembly, Windshield Header - Replace.............. B3490 .6

Read, Initial & Pass On Service Supervision Parts Accounting

LABOR OPERATION TIME LABOR OPERATION DESCRIPTION NUMBER ALLOWANCE --------------------------- ------ --------- Bow, Feature Strip - R&R or Replace....................... B3510 .3 ADD: A - To Replace Retainer .2

Backlight Assembly With Zipper............................ B355O 3.0 (Folding Top Back Curtain)-Replace ADD: A - To Replace Zipper .5

Cover Assembly, Folding Top............................... B3590 4.0 (Less Backlite Assembly)-Replace .4 ADD: A - To Replace Stay Pads (Each)

Boot Assembly, Folding Top - Replace...................... B3610 .2

Bolts, Fasteners and Fittings - Tighten................... B3990 .2

Switch, Folding Top - Replace............................. N2233 .2

Relay, Folding Top - Replace.............................. N2855 .3

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.