LOOSE SHIFTER KNOB REWORK EXISTING SET SCREW HOLE. Pontiac J2000 1982

For 1990-2009 cars

# LOOSE SHIFTER KNOB REWORK EXISTING SET SCREW HOLE

CIMARRON MANUAL TRANSMISSION SHIFTER KNOB LOOSE A MANUAL TRANSMISSION SHIFTER KNOB THAT WORKS LOOSE ON A 1982 CIMARRON CAN BE TIGHTENED BY TAPPING THE EXISTING SET SCREW HOLE WITH A 6M TAP (6-1.00) AND INSTALLING A 6M SET SCREW. NO OVERSIZE DRILLING IS NECESSARY. FOR WARRANTY PURPOSES, USE OPERATION NO. K1040 AT 0.2 HOUR.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.