WIRE WHEEL COVERS LOOSE FIT REPLACEMENT WHEEL COVERS. Pontiac LeMans 1983

For 1990-2009 cars

# WIRE WHEEL COVERS LOOSE FIT REPLACEMENT WHEEL COVERS

THE ABOVE MENTIONED VEHICLES EQUIPPED WITH 14" WIRE WHEEL COVERS MAY HAVE A CONDITION WHERE ONE OR MORE WIRE WHEEL COVERS MAY ROTATE ON THE WHEEL. IF THIS CONDITION IS ENCOUNTERED, INSPECT ALL FOUR (4) WHEEL COVERS FOR THE TYPE OF RETENTION DESIGN. IF THEY HAVE THE FIVE (5) INDIVI- DUAL CLIP DESIGN (SEE VIEW A IN ILLUSTRATION), ALL THE WHEEL COVERS MUST BE REPLACED. A NEW WIRE WHEEL COVER WITH A CONTINUOUS STEEL BAND (SEE VIEW B IN ILLUSTRATION) WENT INTO PRODUCTION ON APPROXIMATELY JANUARY 1, 1983 AND ARE AVAILABLE AT WDDGM (PART NUMBER 10023894). ALL OLD FIVE (5) CLIP DESIGN WIRE WHEEL COVERS MUST BE RETURNED TO I.T.T. THOMPSON, 800 N. LIVINGSTON, MADISON, FLORIDA 32340, ATTENTION: BILL ADAMS. (SEE ILLUSTRATION)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.