REAR WINDOW DEFOGGER GRID LINE VARIATIONS. Pontiac LeMans 1988

For 1990-2009 cars

# REAR WINDOW DEFOGGER GRID LINE VARIATIONS

#### VEHICLES AFFECTED: ALL 1989-90 "A" CARS

The tool numbers have been revised for the fuel level meter assembly spanner wrenches listed in Section "6C", "Engine Fuel" of the 1989-1990 "A" car Service Manuals. The new tool numbers are listed below:

All "A" cars except for the Pontiac 6000 All Wheel Drive (AWD) models .................................. J 36608

Pontiac 6000 All Wheel Drive (AWD) models ........... J 35731

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.