NO REVERSE GEAR ENGAGEMENT (REPAIR DESCRIBED). Pontiac LeMans 1988

For 1990-2009 cars

# NO REVERSE GEAR ENGAGEMENT (REPAIR DESCRIBED)

NO REVERSE GEAR ENGAGEMENT

#### MODELS AFFECTED 1988 LEMANS WITH MANUAL TRANSMISSION ---------------

Some of the subject vehicles may exhibit a condition of "no reverse gear engagement".

This condition may be the result of insufficient clamping force of the "tube to rod" clamp (See Figure 1) caused by an interference condition at the clamp.

The repair action is to replace the clamp, tube front to rod, P/N 90217840 and reinstall bolt and washer.

Re-adjust shift linkage and tighten clamp following service manual procedures.

Labor Operation Number: T1276

Labor Time : .5 Hour

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.