WATER IN OPERA LAMPS FILL WITH BODY CAULK. Pontiac LeMans 1981

For 1990-2009 cars

# WATER IN OPERA LAMPS FILL WITH BODY CAULK

CONDITION: WATER MAY ACCUMULATE BEHIND THE OPERA LAMP LENS ON THE 1981 GRAND PRIX BROUGHAM WITH VINYL TOP. CAUSE: THE WATER ENTERS THROUGH THE SCREW SHOWN IN FIG. 1. CORRECTION: 1.REMOVE OPERA LAMP LENS BY REMOVING BOTTOM SCREW. 2.REMOVE MOULDING RETAINING SCREW. 3.APPLY A SMALL AMOUNT OF FLEXIBLE BODY CAULK IN THE SCREW HOLE, THEN REPLACE THE SCREW. 4.REPLACE THE LENS. FOR WARRANTY PURPOSE, USE OPERATION NUMBER N1564 USING .2 HRS. THIS LABOUR ONLY CLAIM REQUIRES ZONE APPROVAL.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.