ENGINE STARTABILITY COLD/DAMP (NEW DISTRIBUTOR CAP RELEASED). Pontiac LeMans 1992

For 1990-2009 cars

# ENGINE STARTABILITY COLD/DAMP (NEW DISTRIBUTOR CAP RELEASED)

#### SUBJECT: ENGINE STARTABILITY/PERFORMANCE WHEN COLD OR DAMP (NEW DISTRIBUTOR CAP FOR SERVICE)

#### VEHICLES AFFECTED: 1992 LE MANS 'T' CAR W/1.6L (VIN CODE 6)

Recently a new distributor cap, P/N 10457153 was released for service, on 1992 Pontiac Lemans 'T' cars, replacing P/N 10467543. The new cap has aluminum terminals instead of zinc plated iron terminals, for increased durability. The aluminum terminals will provide increased terminal corrosion protection and will result in better startability/performance in cold or damp weather conditions. Whenever a service diagnosis determines that the distributor cap should be replaced, P/N 10457153 should be used.

Replacement of the distributor cap should be performed according to the Pontiac LeMans Service Manual procedure.

For vehicles being repaired under warranty use:

Labour Operation Number: J4360

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.