SMU SECT.0B MAINTENANCE & LUBRICATION-TRANSAXLE OIL. Pontiac LeMans 1990

For 1990-2009 cars

# SMU SECT.0B MAINTENANCE & LUBRICATION-TRANSAXLE OIL

SERVICE MANUAL UPDATE SECTION 0B -------------------------

THIS BULLETIN AMENDS INFORMATION FOUND IN MAINTENANCE AND LUBRICATION (SECTION 0B) OF THE 1989, 1990 AND 1991 PONTIAC LEMANS SERVICE MANUALS (S-8910-T, S-9010-T AND S-9110-T RESPECTIVELY.

THE MANUAL TRANSAXLE FLUID REFERRED TO UNDER " RECOMMENDED FLUIDS AND LUBRICANTS" ON PAGE 0B-7 SHOULD READ MANUAL TRANSAXLE FLUID GM P/N 1 2345371, OR EQUIVALENT. DO NOT USE SYNCHROMESH TRANSAXLE FLUID, GM P/N 12345349.

DISCLAIMER

COPYRIGHT 1991 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.