OIL PAN GASKET LEAKS OIL INSTALL NEW PAN GASKET. Pontiac LeMans 1992

For 1990-2009 cars

# OIL PAN GASKET LEAKS OIL INSTALL NEW PAN GASKET

#### SUBJECT: OIL PAN GASKET OIL LEAKS (INSTALL NEW OIL PAN GASKET)

#### VEHICLES AFFECTED: 1992 PONTIAC LE MANS WITH 1.6L ENGINE

Recently a new oil pan gasket, P/N 90409693 replacing P/N 90353156 was released for production for increased engine durability for the 1992 Pontiac LeMans. The new gasket is polymer coated to prevent oil leakage at the gasket interface. Whenever it becomes necessary to replace the oil pan gasket, the new polymer coated gasket should be used.

Gasket replacement should be performed according to the LeMans Service Manual procedure.

For vehicles being repaired under warranty use:

Labour Operation Number: J1000

Labour Time: 1.4 Hour

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.