DIESEL HEAD GASKET INFORMATION. Pontiac Parisienne (Canada) 1982

For 1990-2009 cars

# DIESEL HEAD GASKET INFORMATION

1982 5.7L V8 DIESEL ENGINES HAVE BEEN ASSEMBLED WITH BOTH FEL-PRO AND GOETZE HEAD GASKETS. THE FEL-PRO HEAD GASKET HAS A DARK BODY, A METAL RING AROUND THE BORE AND BLUE SEALER AROUND THE WATER PASSAGES. THE GOETZE HEAD GASKET HAS A BROWN BODY, A GOLD COLORED METAL RING AROUND THE BORE, BUT DOES NOT HAVE SEALER AROUND THE WATER PASSAGES. SECOND BULLETIN THE DIESEL GASKETS LISTED BELOW WILL SUPERSEDE PREVIOUS GASKETS FOR SERVICING 5.7 LITER DIESEL ENGINES. THESE HEAD GASKETS ARE THE SAME GASKETS CURRENTLY RECOMMENDED FOR USE WITH .030" OVERSIZE PISTONS AND WILL NOW BE USED FOR ALL APPLICATIONS. THE USE OF THESE GASKETS ON STANDARD ENGINES SHOULD PREVENT THE POSSIBILITY OF LOSS OF COMPRESSION DUE TO THE GASKET SEALING RING "FALLING" INTO THE COMBUSTION CHAMBER. THIS SUPERSESSION WILL ALSO AFFECT APPROPRIATE GASKET KITS. COLOR OF SEAL PART NUMBER MODEL YEAR DIAMETER THICK GREY 22519416 78,79,80,83 .030 O.S. +.005 PURPLE 22510719 81,82 .030 O.S. STD

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.