HES. ON ACCEL. MANUEVERS NEW PROM AND EGR VALVE. Pontiac Parisienne (Canada) 1985

For 1990-2009 cars

# HES. ON ACCEL. MANUEVERS NEW PROM AND EGR VALVE

1985 PARISIENNE SEDAN MODELS WITH 4.3L V6 (LB4) ENGINE (VIN CODE Z)

Some 1985 Parisienne models with 4.3L Throttle Body Injection (TBI) engines may experience a hesitation on a tip-in acceleration maneuver. This condition may occur during warm-up or after the vehicle has reached normal operating temperature.

This condition can be corrected by installing a new service PROM as listed below. Federal vehicles also require a new EGR valve.

#### PARTS INFORMATION

EMISSION SYSTEM TRANSMISSION PROM EGR VALVE --------------- ------------ ---- --------- Federal 3-Speed Automatic 1227923 17111577 Federal 4-Speed Automatic 1227922 17111577 California 3-Speed Automatic 1227923 NOT REQUIRED California 4-Speed Automatic 1227922 NOT REQUIRED

WARRANTY INFORMATION

Use applicable labor operation.

SERVICE DEPARTMENT PONTIAC DIVISION GENERAL MOTORS CORPORATION

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.