EGR VALVE OVERRIDE RELAY PRODUCTION CHANGE. Pontiac Parisienne (Canada) 1981

For 1990-2009 cars

# EGR VALVE OVERRIDE RELAY PRODUCTION CHANGE

A RECENT PRODUCTION CHANGE WAS MADE ON 1981 MODELS EQUIPPED WITH LD5 V6 ENGINES. THIS CHANGE CONSISTS OF THE ADDITION OF A JUMPER HARNESS AND A RELAY WHICH ALLOWS THE EGR SOLENOID ELECTRICAL CIRCUIT TO BE OVER RIDDEN UNDER CERTAIN OPERATING CONDITIONS. REFER TO FIGURE 1 AND 2.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.