LO AND REVERSE CLUTCH PISTON SERVICE MANUAL CORRECTION. Pontiac Parisienne (Canada) 1985

For 1990-2009 cars

# LO AND REVERSE CLUTCH PISTON SERVICE MANUAL CORRECTION

ALL 1985 THM 700-R4 TRANSMISSIONS

1985 Service Manuals using the THM 700-R4 Automatic Transmission section should be updated with the information contained in this bulletin.

The Lo & Reverse Clutch Piston dimensions should be 60.92mm (2.398") for the following 1985 Models: PR, MT, VC, PQ, ML, MP, MS, T7. The dimension for ALL OTHER 1985 Models should be 56.52mm (2.225").

Refer to illustration to update your 1985 Service Manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.