ENGINE COOLANT FAN INFORMATION. Pontiac Phoenix 1982

For 1990-2009 cars

# ENGINE COOLANT FAN INFORMATION

WHEN PERFORMING ENGINE COOLANT FAN ELECTRICAL DIAGNOSIS, IT IS IMPORTANT THAT THE TECHNICIAN BE AWARE THAT EACH ENGINE HAS DIFFERENT ELECTRICAL WIRING FOR THE FAN. VARIOUS SYSTEMS MAY BE FOUND ON THE FOLLOWING PAGES OF THE 1982 CHASSIS SERVICE MANUAL: 'A' COOLANT FAN, L-4 PAGE 8A-148, 149 COOLANT FAN, V-6 GASOLINE 8A-144 TO 147 COOLANT FAN, V-6 DIESEL 8A-150 TO 152 'X' COOLANT FAN, L-4 AND V-6 8A-326, 327 COOLANT FAN, H.D., V-6 8A-328, 329

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.