REVISED PROCEDURE TO CHECK TRANSAXLE OIL LEVEL-125C. Pontiac Phoenix 1983

For 1990-2009 cars

# REVISED PROCEDURE TO CHECK TRANSAXLE OIL LEVEL-125C

THE PROCEDURE EXPLAINING "CHECKING TRANSAXLE OIL LEVEL" SHOWN ON PAGE 7A-2, SECTION 7A OF THE FOLLOWING SHOP MANUALS IS INCORRECT: 1983 CELEBRITY SHOP MANUAL ST-370-83 1983 CITATION SHOP MANUAL ST-365-83 1983 CAVALIER SHOP MANUAL ST-366-83 STEP 1 SHOULD READ: "IF IT FELT COOL OR WARM, ABOUT ROOM TEMPERATURE AND WARMER, BUT NOT TOO HOT TO HOLD, THE LEVEL SHOULD BE BETWEEN THE TWO DIMPLES ABOVE THE "FULL" MARK. STEP 3 SHOULD READ: IF IT WAS TOO HOT TO HOLD, THE LEVEL SHOULD BE IN THE CROSS HATCHED AREA ON THE DIPSTICK, NEAR THE "FULL" MARK.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.