TRAILERING CAPACITIES MAX. RECOMMENDED WEIGHTS. Pontiac Phoenix 1983

For 1990-2009 cars

# TRAILERING CAPACITIES MAX. RECOMMENDED WEIGHTS

The following is a preliminary listing of trailering capacities for 1983 Pontiac vehicles. These are the maximum recommended weights.

TRAILERING CAPACITY MODEL KG (LBS.) COMMENTS ----- --------- -------- 1000 454 (1000) -

2000 454 (1000) -

FIREBIRD 454 (1000) L4 907 (2000) V6 & V8

PHOENIX 454 (1000) L4 907 (2000) V6

6000 454 (1000) L4 & DIESEL 907 (2000) V6

GRAND PRIX 907 (2000) DIESEL; V6+2.73 AXLE; BONNEVILLE V8 GAS+2.29 AXLE

1361 (3000) V6+3.08 AXLE

1814 (4000) V6+3.23 AXLE V8 GAS+2.73 AXLE

2267 (5000) V8 GAS+3.08 AXLE

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.