PROTRUDING SEAT SPRINGS SEAT OPTION AM6/AV7 - REPAIR. Pontiac Safari Wagon 1989

For 1990-2009 cars

# PROTRUDING SEAT SPRINGS SEAT OPTION AM6/AV7 - REPAIR

#### VEHICLES AFFECTED: 1986-89 B-CARS

This bulletin is being released to repair front seat cushions which may have seat wire protruding through the foam. The protrusion is located at the rear outboard area of the seat cushion (See Illustration).

#### Procedure:

1. Remove seat from vehicle and seat cover from cushion. (See seat Section Body Service Manual).

2. Slit foam cushion to expose wire as illustrated. (See seat Section Body Service Manual).

3. Clip off end of wire as illustrated in view "A", remove and discard this piece.

4. Push wire down into foam cushion and glue slit in cushion together with 3M 08080 General Trim Adhesive or equivalent.

5. Install seat cover (new if needed) and seat to vehicle.

Use most applicable Labour operation and time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.