LIMITED SLIP REAR AXLE LUBRICANT RECOMMENDATIONS. Pontiac Safari Wagon 1987

For 1990-2009 cars

# LIMITED SLIP REAR AXLE LUBRICANT RECOMMENDATIONS

ALL 1987 REAR DRIVE PASSENGER CARS WITH LIMITED-SLIP DIFFERENTIALS

"Please discard bulletin 87-7-3. This bulletin was put in Section 7 in error and the part numbers were incorrect."

Several changes have been made to the limited-slip rear axle lubricant service change recommendations.

The following information may not be reflected in all 1987 service manuals, update as necessary.

LIMITED-SLIP DIFFERENTIAL LUBRICATION

#### MODEL APPLICATIONS LUBRICANT ADDITIVE ----- ------------ --------- -------- Safari Wagon All 1052271 1052358

Grand Prix All 1052271 Do Not Use

Firebird Rear Disc Brakes 1050010 Do Not Use

Firebird All Others 1052271 Do Not Use

Safari Wagon models require a lubricant change at 7,500 miles.

Firebird and Grand Prix models require a lubricant change at 7,500 miles only if they are used for pulling a trailer.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.