HIGHER THAN NORMAL IDLE CHECK MANIFOLD VAC FITTING CAP. Pontiac Sunbird 1987

For 1990-2009 cars

# HIGHER THAN NORMAL IDLE CHECK MANIFOLD VAC FITTING CAP

1987 SUNBIRD MODELS EQUIPPED WITH OHC 4 ENGINE (VIN CODE K) WITHOUT A/C AND WITHOUT CRUISE CONTROL

Customer vehicles that exhibit a higher than normal idle RPM and have no A/C or cruise control should be checked for a vacuum leak at the intake manifold vacuum fitting.

Vehicles between the following VINS:

KlH7593965 to KlH7602202

have an incorrect vacuum cap that should be replaced by P/N 343350, which is available from GMSPO.

Warranty Information

Labor Operation: J6980

Labor Time : .2 hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.