DRIVE AXLE TRI-POT SEAL CLAMP PART NUMBERS. Pontiac Sunbird 1986

For 1990-2009 cars

# DRIVE AXLE TRI-POT SEAL CLAMP PART NUMBERS

1986 4-CYLINDER NON TURBO SUNBIRD VEHICLES

"Please discard bulletin 86-4-1, dated 10/86 due to updated information included in this bulletin."

For the 1986 model year, a limited quantity of 4-cylinder, non turbo Sunbird vehicles with both automatic and manual transaxles have been built using a low-profile, earless Tri-Pot seal retaining clamp on the left-hand inboard axle joint.

These assemblies may be serviced with Seal Service Kit Tri-Pot 7845350 (which contains standard clamp 7843226) using tool J 35910 Drive Axle Seal Clamp Pliers (refer to Figure 1).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.