REPAIR PROCEDURE MANUAL TRANS. AXLE CLUTCH START SWITCH. Pontiac Sunbird 1984

For 1990-2009 cars

# REPAIR PROCEDURE MANUAL TRANS. AXLE CLUTCH START SWITCH

WHEN REPAIRING THE CLUTCH START SWITCH WIRE TERMINALS, THE CONNECTOR SHOULD BE INSTALLED AND THE WIRES SECURED WITH A TIE STRAP TO THE SWITCH BODY AS SHOWN IN ILLUSTRATION. THIS WILL MINIMIZE WIRE MOVEMENT AT THE TERMINALS.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.