ENGINE COOLANT TEMP. GAGE READING/CORRECT INDICATION. Pontiac Sunbird 1988

For 1990-2009 cars

# ENGINE COOLANT TEMP. GAGE READING/CORRECT INDICATION

#### Models Affected: 1986-90 SUNBIRD WITH 2.0L

The engine coolant temperature gage contains five indicator or "tick" marks. The first mark is labeled 40 degree C or 100 degree F. The 1/4 mark is not labeled but corresponds to 90 degree C or 190 degree F. The 1/2 mark is not labeled but corresponds to 105 degree C or 220 degree F, and the 3/4 mark corresponds to 115 degree C or 240 degree F. The last indicator mark is labeled 130 degree C or 260 degree F.

Both engines, the 2.0L (VIN K) and the 2.0L (VIN M), use a 90 degree C (190 degree F) engine coolant thermostat. Therefore, the "normal" pointer position for the engine coolant temperature gage is at the 1/4 indicator mark, or slightly higher for normal operating conditions.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.